Date created: 09/11/2017

**MGCC\_MdlMgmt**

This is the MGCC project model management part. The major purpose of this VI is to adapt the feeder information from “SHE215.xslx”.

1. Since there is no while loop here, there is no need for watchdog timer.
2. There are two complex array here. Thus a new data type “c” for complex is updated in the name convention.
3. 2d double array is created here as a new data tye.
4. Since math script does not support 3d array, for BLIN and ZLIN, three separate math scripts are utilized here.
5. For other detailed issues, please refer to the readme.txt